IMU – Inertial Measurement Unit

AIRtouch – Artificial, Intelligent Remote touch keyboard

USB – Universal Serial Bus

MSP430 – Mixed Singnal Processor 430

FSR – Force Sensetive Resister

PCB – Printed Circuit Board

UART – Universal Asynchronious Receive Transmit protocol

PWM – Pulse Width Modulation

TL – Thumb Left

TR – Thumb Right

PLX-DAQ - Parallax Data Acquisition Tool

COM – Communication

CSV – Comma Separated Values

RTC – Real Time Clock

I/O – Input and Output

ASCII - **American Standard Code For Information Interchange**

RI – Right Index finger

RM – Right Middle finger

RR – Right Ring finger

RL – Right Little finger

LI – Left Index finger

LM – Left middle finger

LR – Left Ring finger

LL – Left Little finger

UL – Upper Layer(U)

ML – Middle Layer(M)

LL – Lower Layer(L)